1. Practical. Configure EDA60 so that when reading a QR code it takes the first group of characters until it finds a comma, other characters are then discarded. This should work just for QR codes.
2. Can you use cellular data when there is no Wi-Fi on a CN50 (32 GB, Numeric, WWAN).

Yes.

1. What would be the biggest restriction when creating a bar code on Enterprise Provisioner to download and then install an application into a device?

Both Enterprise Provisioner and the device must be connected to the same network.

1. Name 3 tasks you can perform with bar codes generated using Enterprise Provisioner.

* Connecting to a network.
* Factory reset a device.
* Download and install an application.
* Device Settings.
* Run an app.
* OS Updates.
* Reboot.

1. Normally licenses when generated are exported into two different type of files, which are these?

.xml and .pdf.

1. Honeywell apps per platform (Windows/Android). Specify name of pack and apps on each pack.

Windows.

Intermec Client Pack (Intermec Terminal Emulator, Intermec Browser, Intermec Launcher).

Android.

Software Client Pack (Honeywell SmartTE, Honeywell Enterprise Browser, Honeywell Launcher).

1. What is the most effective and recommended way to recover information in our device when AppLock credentials have been forgotten?

There is no way to recover information when credentials have been forgotten.

1. What are the two ways to enable OCR?

By scanning the OCRENA1 barcode.

Sending the command via EZConfig.

1. What server instance is recommended to install alongside Staging Hub?

Windows Server SQL (Any version above 2008).

1. What is the wild card character usable in white listing URL to add subsequent URLs?

Percent symbol.

1. Encryption method used to encrypt Enterprise Browser and Launcher passwords?

SHA256.

1. What type of reset must be performed if the Dubai terminal is downgraded from Android O to Android N?

Enterprise Reset.

1. Applications built for Android P can use either HTTP or HTTPS for browsing?

False.

1. Which two imagers will be available for the EDA71?

N3601 and N6703.

1. EDA71 offers a WWAN radio option?

True.

1. CK65 scan engines available are:

N6703 and EX20.

1. What would happen if you remove the battery of a CK65 while using Honeywell Enterprise Browser?

Nothing. Device has the energy to sustain the system for 3 minutes after a battery swap. After that device will just turn off.

1. What is PCAP feature on a touchscreen?

In indicates that the touchscreen is multitouch.

1. How many multi-touch points does PCAP support?

5-point multitouch.

1. Practical. Company has a massive warehouse, since the are is so big they are planning to use VM1A’s GPS to locate the items when collecting/placing them. Additionally, they want to pair 8680i scanners using NFC to help the scanning process. What will be an issue in this case?

Also. Since they are using NFC they need to know what Bluetooth class the device supports.

VM1A will not have WWAN, thus NO GPS. Bluetooth class is 5.0.

1. What is the maximum size for a SD Card in a VM1A?

512 GB.

1. Name 3 new features on Android 8.

* PIP.
* Autofill framework.
* Improved battery menu.
* Bluetooth battery level and info.
* Rescue party: No more boot loops.
* Install from unknown sources is missing.
* Notification dots.

1. How does PIP (picture in picture) works?

Allows to play a video on a floating screen while browsing the device out of the video application.

1. What tool inside Power Tools will let us know the IP Address, MAC Address, RSS of our device/connection?

Wi-Fi Diagnostics.

1. What does the HUpgrader utility do?

Allows user to update kernel on products using the Mobility Edge Platform

1. In Android you can know if a kernel is GMS or Non-GMS by checking the first two numbers of the kernel. Select the correction options for Android 7:

* …83 Non-GMS - …84 GMS.
* …83 GMS - …84 Non-GMS.
* …88 Non-GMS - …87 GMS.
* …88 GMS – 87 Non-GMS.

1. Scanner N6603SR is used in which of the following devices:

* EDA51
* CT40
* CT50
* CT60
* CN80
* CK75

1. CK71 offers two scan engine options (EX25 and N5603ER). Select the correct description for each scan engine:

* EX25 near-far 2D area imager / N5603ER extended range 2D imager.
* EX25 extended range 2D imager / N5603ER near-fear 2D area imager.

1. Match the scan engine with the beam they produce (These scan engines are present on CK71, CN70 devices).

* N5603
* EA30
* EX25
* EV12

1. What power option has the following description: Radars off, screen and blacklight off, will turn on with power button only:

* Suspend
* Hibernate
* Shutdown

1. Match power options with their proper description:
2. Screen off
3. Suspend
4. Hibernate
5. Shut down

\_b\_ Radios are still on, screen and blacklights are off, turn back on with power button only.

\_d\_ Everything is off. Will boot up with power button.

\_a\_ Processors and radios still running, screen and blacklight are off, turns back on with any key press or screen tap.

\_c\_ Radios off, screen and blacklight off, will turn on with power button only.

1. What is the name of the key with the “?” symbol on the CK70 and what does it do?

“Device Health Key”. Gives information about battery, system, connections, firmware version, etc.

1. What is SNR and what information does it provide?

“Signal to Noise Ratio”. Shows data rate and channel.

1. Describe Intermec Browser.

Uses web-based applications but want to control their users’ access to the web.

1. Describe Intermec Launcher.

Configurable locked-down menu program that prevents end-user from accessing start menu and non-authorized apps. End-user log in and they access only authorized programs.

1. Describe Intermec Terminal Emulator.

Is the next generation of Intermec popular terminal emulation client designed for Enterprise level data collection. User interface and a common menu structure to use and management of applications running on Intermec.

1. What’s the name of the bundle in which all the Honeywell application for Windows are located.

Intermec Client Pack

1. Honeywell apps for Android are divided into three main bundles. Name them:

* ECP (Enterprise Client Pack)
* SCP (Software Client Pack)
* DCP (Device Client Pack)

1. Practical. Explain how to replicate configuration from one CK65 to another, using just the device and a computer, no software (like Enterprise Provisioner).

Go to Power Tools, go to EZConfig, on the hamburger select Generator. Then the DeviceConfig.xml is going to be generated.

Browse device on computer, copy that file, save it to the computer. Then plug the new device in which you want to have the configuration. Browser that device and copy the file into the same folder.

1. Practical. While at the office, Ron generated a code on Enterprise Provisioner which enables provisional mode and then downloads and installs an apk. All the employees at facility used the code on their devices and were able to get the application.

Jose, who was at home that day tried to read the code with his device (He is using the same device, same version, configuration). His devices beeps but nothing happens. He then did a factory reset expecting that to fix the issue, it didn’t.

What is the problem in this scenario?

He is connected to a different Network from where the application is stored.

1. What is the tool inside Power Tools used to generate the configuration .xml for the device?

EZConfig.

1. Among all the xml files generated using EZConfig which is the file in which you can get the configuration of the device?

DeviceConfig.xml.

1. What is the only restriction when changing OS from Android 6 to Windows 6.5

In units with Android 6 already loaded from factory is not possible to load Windows 6.5. If the device has been converted to Android 6 it is possible to go back to Windows 6.5.

1. Can you generate a license directly on Staging Hub using the Activation ID?

True.

1. Sometimes when switching between networks the IP in Enterprise Provisioner remains with the same IP. In Windows, how can we verify if the IP of our computer is the one that Enterprise Provisioner is showing?

Checking IP with cmd. Then ipconfig.

1. How do we check which keyboard map we need to add to SmartTe when working with a specific device?

Using the number displayer in SmartTE in our device, then the keyboard map should have that number in the name.

1. What is a MDM and what would be an example?

Mobile Device Management. For example, Staging Hub.

1. What is Staging Hub.

Staging Hub gives you a consistent and centralized plaftorm so that you can easily manage and monitor your deployed Honeywell devices, such as mobile computers, printers, RFID readers, and other peripheral and network devices.

1. When using SmartTE and working locally on a computer, what is the most common name we give to our server?

localhost.

1. Using Enterprise Provisioner, is it possible to generate a code to set provisioning mode active all the time in a device? Even if the device is restarted.

True.